BBC Master 128 Cartridge Interface

This application note details the Cartridge Interface on the Master Series machines with differences for operation with the Electron Plus 1 noted where relevant.

Applicable Hardware : BBC Master 128

Support Group Acorn Computers Limited Acorn House Vision Park Histon Cambridge CB4 4AE

Related Application Notes:

Copyright ' Acorn Computers Limited 1992

Every effort has been made to ensure that the information in this leaflet is true and correct at the time of printing. However, the products described in this leaflet are subject to continuous development and improvements and Acorn Computers Limited reserves the right to change its specifications at any time. Acorn Computers Limited cannot accept liability for any loss or damage arising from the use of any information or particulars in this leaflet. ACORN, ECONET and ARCHIMEDES are trademarks of Acorn Computers Limited.

3rd August 1992

Support Group Application Note Number: 035 Issue: 1 Author: D J Bell

Abbreviations

Abbreviations are used in this Note as follows: A/L Active Low O/C Open Collector output CMOS Complementary-symmetry Metal Oxide Semiconductor CPU Central Processor Unit ie, the microprocessor TTL Transistor-Transistor Logic & A hexadecimal number follows n As a signal prefix means Active Low output (A/L) PCB Printed Circuit Board NMOS Nitride-layer Metal Oxide Semiconductor

Cartridge Orientation

The cartridge pinning in the Master Series machine is arranged as follows:

Components are normally mounted onto Side A of the PCB within the cartridge.

Pinout

Pins are described viewed from "within" the cartridge ie, an "Input" is an input to the cartridge. An "output" is an output to the computer.

SIDE A 1 +5V - Logic power supply. 150mA max in a Master with co-processor fitted and with disk drives. 50mA max in an Electron Plus 1.

2 nOE - Output Enable. Input from A/L CMOS level. Low during PH12 period of system clock. It is intended to switch on the output buffers of cartridge memory devices. It is not guaranteed low at other times.

3rd August 1992

Support Group Application Note No. 035, Issue 1

Support Group Application Note No. 035, Issue 1

Viewed from above

Pin 22 Pin 1

Side A Side B

Side A Side B

Front 0

3 nRST - System Reset. Input from A/L CMOS level. Low during a system reset. It is not synchronised to any clock.

4 CSRW - Chip Select - Read/Write. Input from CMOS level. Master - Changes function according to the memory region that the CPU is addressing. During accesses to &FC00 through &FEFF it is equivalent to the CPU Read/Write line during nPH12. For all other accesses it is an Active High chip select for memory devices. It is not guaranteed low at other times. Electron - CPU Read/Write line.

5 A8 - Address line 8. Input from TTL level.

6 A13 - Address line 13 Input from TTL level.

7 A12 - Address line 12 Input from TTL level.

8 PH12 - CPU clock. Input from CMOS levels. Computer’s PH12 output.

9 -5V - Negative supply voltage. 20mA max. This -5V may not be available on all Acorn Cartridge Interfaces. To ensure compatibility, negative voltages should be generated within the Cartridge if required.

10 CSYNC/MADET Master - There are two functions dependent upon link 12 in the computer: E/nB - the default function. It enables cartridges to know which machine they are plugged into. It is connected to 0V in the Master (and unconnected in the Electron). Link 12 is set to position B. CSYNC - Composite Sync. Input from TTL levels. System Vertical & Horizontal sync is made available fro Genlock use. Set Link 12 to position B. Electron - Unconnected.

11 RNW/READY Master - R/W - Data Direction Control. Input from TTL levels System data buffer direction control. If low, cartridges are being written to; if high and selected, they may drive the bus during PH12. Electron - READY - CPU wait state control O/C A/L output When driven low, this line will cause the CPU to extend it’s cycle until READY is released. Only works with CMOS CPUs. Will only work on READ cycles with NMOS CPUs.

12 nNMI - Non-maskable Interrupt. O/C A/L output. Connected to the system NMI line.

13 nIRQ - Interrupt request. O/C A/L output. Connected to the system IRQ line.

3rd August 1992

Support Group Application Note No. 035, Issue 1

Support Group Application Note No. 035, Issue 1

14 nINFC - Internal Page &FC Input from TTL levels. A/L. Memory Active decode input. Master - When bit IFJ in the Master ACCON register (via &FE34) is set, all accesses to &FC00 through &FCFF will cause this select to become active. Electron - Not applicable.

15 nINFD - Internal Page &FD Input from TTL levels. A/L. Memory Active decode input. Master - When bit IFJ in the Master ACCON register (via &FE34) is set, all accesses to &FD00 through &FDFF will cause this select to become active. Electron - Not applicable.

16 ROMQA - Memory paging select Input from TTL levels. This is the least significant bit of the ROM select latch located at &FE30 in the Master, and at &FE05 in the Electron.

17 Clock Input/Output TTL levels. Master - Links on the computer select one of two functions: a) 16Mhz Output to computer (Link DB only). b) 8 Mhz Input to cartridge (Link CD in addition to AB).

The user should ensure that the links are set correctly, and that there is proper termination. Normally only AB is linked in the computer. WARNING! If Link AB in the computer is removed, the dynamic RAM could be damaged unless a clock supply is fed into the computer AT ALL TIMES whilst the computer is powered. The user must ensure that the Cartridge cannot be removed by accident and interrupt the clock supply. The use of this clock facility must be at the users risk. Electron - 16 Mhz input.

18 nROMSTB/nCRTCRST TTL levels. Master - nCRTCRST is an Active Low Output signal of the system CRTC reset input. It is provided for Genlock use. Electron - nROMSTB is an Active Low Input which selects &FC73. It is intended to be used as a Paging Register.

19 ADOUT - System audio output. Filtered output of the sum of all audio inputs to the computer. No significant load should be taken from this pin.

20 AGND - Audio Ground. The zero volt return for ADOUT. It should be used instead of system 0V to minimise audio noise.

21 ADIN - Cartridge audio input. Master - An output to the computer’s audio circuitry. It "sees" an impedance of at least 1K ohm. Only one cartridge using this output should be connected to the computer at one time. Electron - This is a connection from one cartridge to another.

22 0V - Zero volts. System earth return for digital signals.

3rd August 1992

Support Group Application Note No. 035, Issue 1

Support Group Application Note No. 035, Issue 1

SIDE B 1 +5V - Logic power supply. 150mA max in a Master with co-processor fitted and with disc drives. 10mA max in an Electron Plus 1.

2 A10 - Address line 10. Input from TTL levels.

3 D3 - Data bus line 3. Input/Output TTL levels.

4 A11 - Address line 11. Input from TTL levels.

5 A9 - Address line 9. Input from TTL levels.

6 D7 - Data bus line 7. Input/Output TTL levels.

7 D6 - Data bus line 6. Input/Output TTL levels.

8 D5 - Data bus line 5. Input/Output TTL levels.

9 D4 - Data bus line 4. Input/Output TTL levels.

10 nOE2/LPSTB - O/P Enable/Light Pen Strobe. Input from TTL levels. Master - With link 21 removed in the computer, this pin provides a connection between the two cartridges. With the link in place, the pin forms a connection to a pull-up resistor in the computer to +5V. The connection is also made to the CRTC Light-Pen Strobe and interrupt structure. Electron - This provides an additional A/L enable for ROMs in the Electron. This corresponds to ROM position 13 and responds quickly to Service Calls. It is low during the A/L portion of PH12. It is not guaranteed high at other times.

11 BA7 - Buffered address line 7. Input from TTL levels. Master - This line holds addresses valid for 125nS after PH12 goes low. Electron - This is not buffered nor held valid for an extended period in the Electron.

12 BA6 - Buffered address line 6. Input from TTL levels. see pin 11.

13 BA5 - Buffered address line 5. Input from TTL levels. see pin 11.

14 BA4 - Buffered address line 4. Input from TTL levels. see pin 11.

15 BA3 - Buffered address line 3. Input from TTL levels. see pin 11.

16 BA2 - Buffered address line 2. Input from TTL levels. see pin 11.

17 BA1 - Buffered address line 1. Input from TTL levels. see pin 11. 5

3rd August 1992

Support Group Application Note No. 035, Issue 1

Support Group Application Note No. 035, Issue 1

18 BA0 - Buffered address line 0 Input from TTL levels. see pin 11.

19 D0 - Data bus line 0. Input/Output TTL levels. 20 D2 - Data bus line 2. Input/Output TTL levels. 21 D1 - Data bus line 1. Input/Output TTL levels. 22 0V - Zero volts. Digital signal Earth return.

3rd August 1992

Support Group Application Note No. 035, Issue 1

Support Group Application Note No. 035, Issue 1