Risc PC Screen Resolutions and Colour Combinations

This Application Note provides a comparison of the Risc PC’s screen resolution capability with existing video standards and older screen mode numbers. The maximum number of colours supported under each standard for a range of current Acorn monitors is also given.

Applicable Hardware : Risc PC 600 series

Support Group Acorn Computers Limited Acorn House Vision Park Histon, Cambridge CB4 4AE

Related Application Notes:

Every effort has been made to ensure that the information in this leaflet is true and correct at the time of printing. However, the products described in this leaflet are subject to continuous development and improvements and Acorn Computers Limited reserves the right to change its specifications at any time. Acorn Computers Limited cannot accept liability for any loss or damage arising from the use of any information or particulars in this leaflet. Acorn, the Acorn Logo, Acorn Risc PC, ECONET, AUN, Pocket Book and ARCHIMEDES are trademarks of Acorn Computers Limited.

ARM is a trademark of Advance RISC Machines Limited. All other trademarks acknowledged. '1994 Acorn Computers Limited. All rights reserved.

None

10th June 1994

Support Group Application Note Number: 262 Issue: 0.3 Author:DW

The following table gives information on the range of Acorn monitors and standard resolutions supported by Risc PC with all VRAM configurations, and examples of typical backward-compatible numbered screen modes which display these resolutions.

The AKF85 can be made to operate in a 1600x1200 screen mode; a suitable Monitor Definition File is available from Acorn Customer Services.

2

10th June 1994

Support Group Application Note No. 262, Issue 0.3

Support Group Application Note No. 262, Issue 0.3

640x256 (CGA)

896x352 (EGA)

640x480 (VGA)

1024x768 (XGA)

1280x1024 1600x1200

800x600 (SVGA)

Resolutions Pixels:

Standard:

Equivalent Screen Modes

12/15 39/40 27/28 31

AKF30/40

AKF50/52

AKF60

AKF85

Video

No VRAM

1Mb VRAM

2Mb VRAM

Monitors

(Letterbox)

32k

256 16

256

256

16M

16M

16M

16M

16 32k

256

32k

32k

32k

32k

32k

Memory

Number of Colours Displayable

- -

- -

Risc PC Screen Resolutions

and Colour Combinations

This Application Note provides a comparison of the Risc PC’s screen resolution capability with

existing video standards and older screen mode numbers. The maximum number of colours

supported under each standard for a range of current Acorn monitors is also given.

Applicable

Hardware :

Risc PC 600 series

Support Group

Acorn Computers Limited

Acorn House

Vision Park

Histon, Cambridge

CB4 4AE

Related

Application

Notes:

Every effort has been made to ensure that the information in this leaflet is true and correct at the time of

printing. However, the products described in this leaflet are subject to continuous development and

improvements and Acorn Computers Limited reserves the right to change its specifications at any time.

Acorn Computers Limited cannot accept liability for any loss or damage arising from the use of any

information or particulars in this leaflet. Acorn, the Acorn Logo, Acorn Risc PC, ECONET, AUN, Pocket

Book and ARCHIMEDES are trademarks of Acorn Computers Limited.

ARM is a trademark of Advance RISC Machines Limited.

All other trademarks acknowledged.

'1994 Acorn Computers Limited. All rights reserved.

None

10th June 1994

Support Group Application Note

Number: 262

Issue: 0.3

Author:DW

The following table gives information on the range of Acorn monitors and standard resolutions supported

by Risc PC with all VRAM configurations, and examples of typical backward-compatible numbered screen

modes which display these resolutions.

The AKF85 can be made to operate in a 1600x1200 screen mode; a suitable Monitor Definition File is

available from Acorn Customer Services.

2

10th June 1994

Support Group Application Note No. 262, Issue 0.3

Support Group Application Note No. 262, Issue 0.3

640x256

(CGA)

896x352

(EGA)

640x480

(VGA)

1024x768

(XGA)

1280x1024 1600x1200

800x600

(SVGA)

Resolutions

Pixels:

Standard:

Equivalent

Screen

Modes

12/15 39/40 27/28 31

AKF30/40

AKF50/52

AKF60

AKF85

Video

No VRAM

1Mb VRAM

2Mb VRAM

Monitors

(Letterbox)

32k

256 16

256

256

16M

16M

16M

16M

16 32k

256

32k

32k

32k

32k

32k

Memory

Number of Colours Displayable

- -

- -

Risc PC Screen Resolutions

and Colour Combinations

This Application Note provides a comparison of the Risc PC’s screen resolution capability with

existing video standards and older screen mode numbers. The maximum number of colours

supported under each standard for a range of current Acorn monitors is also given.

Applicable

Hardware :

Risc PC 600 series

Support Group

Acorn Computers Limited

Acorn House

Vision Park

Histon, Cambridge

CB4 4AE

Related

Application

Notes:

Every effort has been made to ensure that the information in this leaflet is true and correct at the time of

printing. However, the products described in this leaflet are subject to continuous development and

improvements and Acorn Computers Limited reserves the right to change its specifications at any time.

Acorn Computers Limited cannot accept liability for any loss or damage arising from the use of any

information or particulars in this leaflet. Acorn, the Acorn Logo, Acorn Risc PC, ECONET, AUN, Pocket

Book and ARCHIMEDES are trademarks of Acorn Computers Limited.

ARM is a trademark of Advance RISC Machines Limited.

All other trademarks acknowledged.

'1994 Acorn Computers Limited. All rights reserved.

None

10th June 1994

Support Group Application Note

Number: 262

Issue: 0.3

Author:DW

The following table gives information on the range of Acorn monitors and standard resolutions supported

by Risc PC with all VRAM configurations, and examples of typical backward-compatible numbered screen

modes which display these resolutions.

The AKF85 can be made to operate in a 1600x1200 screen mode; a suitable Monitor Definition File is

available from Acorn Customer Services.

2

10th June 1994

Support Group Application Note No. 262, Issue 0.3

Support Group Application Note No. 262, Issue 0.3

640x256

(CGA)

896x352

(EGA)

640x480

(VGA)

1024x768

(XGA)

1280x1024 1600x1200

800x600

(SVGA)

Resolutions

Pixels:

Standard:

Equivalent

Screen

Modes

12/15 39/40 27/28 31

AKF30/40

AKF50/52

AKF60

AKF85

Video

No VRAM

1Mb VRAM

2Mb VRAM

Monitors

(Letterbox)

32k

256 16

256

256

16M

16M

16M

16M

16 32k

256

32k

32k

32k

32k

32k

Memory

N u m b e r o f C o l o u r s D i s p l a y a b l e - -